REQPROD 52687 / -; 2

Tprocedure:

|  |  |
| --- | --- |
| **General:** | REQPROD 52687 / - ; 2 |
| **Title:** | Data Compression Method 1 Parameters |
| **Purpose:** | State the compression method #1 parameters |
| **Description:** | The size of the look-ahead buffer in the LZSS compression method shall be 16 bytes. |
| **Precondition:** | - |

**Test execution:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Test Step | Action (client) | Expected Result (ECU) | Result | Comment |
| 1 | Send: | ECU: |  |  |

|  |  |
| --- | --- |
| **Postcondition:** | - |
| **Description:** | This REQPROD can’t be verified by Testscript need to be verified by Inspection Code. |
| **Path:** | ECU-SW : HVBM SPA2 Base Technologies / MAIN; 2  SWC : HVBM SPA2 Base Technologies / MAIN; 2  [SWC : HVBM SPA2 Software Download / MAIN; 0](eASEE:VCC_EEDM,10980011)  Realizes  [LC : Data Compression & Encryption Specification HVBM SPA2 / -; 0](eASEE:VCC_EEDM,10980534)  [LC : Data Compression & Encryption Specification / -; 3](eASEE:VCC_EEDM,10583077)  Software Component Requirements  Compression Method 1# Requirements  Data Compression  [REQPROD : Data Compression Method 1 Parameters / -; 2](eASEE:VCC_EEDM,10622518) |